FUNCTION NAME eixm_BsqWrite - Write BSQ-formatted image data to the destination medium SYNTAX

#include <eixm_Export.h>

void eixm_BsqWrite( dsc, pstack, width, height, meter, err )

Arguments

Eixm_Descrip *dsc;/* Source description */

Eimg_PixelRectStack *pstack;/* Destination pixelrectstack */
long width;/* Number of columns to write */

long height;/* Number of rows to write */ Emet_MeterInfo *meter;/* Meter info structure */ Eerr_ErrorReport **err;

DESCRIPTION

This function writes a block of BSQ-formatted image data, starting at the current position on the medium, frompstack. You must calleixm_ExportInit before calling this function. If meter is not NULL, the meter percentage will be updated from 0 to 100.

RETURN VALUES No value is returned.

SEE ALSO

eixm_BilWrite eixm_BipWrite

From ERDAS IMAGINE eixm On-Line Help. Copyright (c) 1982-1997 ERDAS, Inc.